<?xml version="1.0"?>
<!-- Autopilot Version 4 Configuration for the Citation-Bravo or -->
<!-- Citation Based on 737-AutopilotV4.XML  -->

<!-- This is still in development, so not all of the controllers are -->
<!-- currently used, or work properly. -->


<PropertyList>

<!-- =============================== -->
<!-- ======  Roll Axis Modes  ====== -->
<!-- =============================== -->

<!-- Wing leveler -->
<pid-controller>
  <name>Wing Leveler (Turn Coordinator based)</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>wing-leveler</value>
  </enable>
  <input>
    <prop>/orientation/roll-deg</prop>
  </input>
  <reference>
    <value>0.0</value>
  </reference>
  <output>
    <prop>/controls/flight/aileron</prop>
  </output>
  <config>
    <Kp>0.5</Kp>        <!-- proportional gain -->
    <beta>1.0</beta>    <!-- input value weighing factor -->
    <alpha>0.1</alpha>  <!-- low pass filter weighing factor -->
    <gamma>0.0</gamma>  <!-- input value weighing factor for unfiltered -->
                        <!-- derivative error -->
    <Ti>10.0</Ti>        <!-- integrator time -->
    <Td>0.00001</Td>    <!-- derivator time -->
    <u_min>-1.0</u_min> <!-- minimum output clamp -->
    <u_max>1.0</u_max>  <!-- maximum output clamp -->
  </config>
</pid-controller>


<!-- Heading Bug Hold.  2 stage cascade controller. -->

<!-- Stage #1 sets target roll based on diff between current heading -->
<!-- and heading bug. -->
<pi-simple-controller>
  <name>Heading Bug Hold (DG based) Stage 1</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>dg-heading-hold</value>
  </enable>
  <input>
    <prop>/autopilot/internal/fdm-heading-bug-error-deg</prop>
  </input>
  <reference>
    <value>0.0</value>
  </reference>
  <output>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </output>
  <config>
    <Kp>-2.0</Kp>        <!-- proportional gain -->
    <Ki>0.0</Ki>         <!-- integral gain -->
    <u_min>-30.0</u_min> <!-- minimum output clamp -->
    <u_max>30.0</u_max>  <!-- maximum output clamp -->
  </config>
</pi-simple-controller>

<!-- Stage #2 drives the ailerons to achieve the desired roll deg. -->
<pid-controller>
  <name>Heading Bug Hold (DG based) Stage 2</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>dg-heading-hold</value>
    <honor-passive>true</honor-passive>
  </enable>
  <input>
    <prop>/orientation/roll-deg</prop>
  </input>
  <reference>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </reference>
  <output>
    <prop>/controls/flight/aileron</prop>
  </output>
  <config>
    <Kp>0.5</Kp>        <!-- proportional gain -->
    <beta>1.0</beta>    <!-- input value weighing factor -->
    <alpha>0.1</alpha>  <!-- low pass filter weighing factor -->
    <gamma>0.0</gamma>  <!-- input value weighing factor for -->
                        <!-- unfiltered derivative error -->
    <Ti>10.0</Ti>       <!-- integrator time -->
    <Td>0.00001</Td>    <!-- derivator time -->
    <u_min>-1.0</u_min> <!-- minimum output clamp -->
    <u_max>1.0</u_max>  <!-- maximum output clamp -->
  </config>
</pid-controller>


<!-- True Heading hold.  2 stage cascade controller. -->

<!-- Stage #1 sets target roll based on diff between current heading -->
<!-- and target heading. -->
<pi-simple-controller>
  <name>True Heading Hold (DG based) Stage 1</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>true-heading-hold</value>
  </enable>
  <input>
    <prop>/autopilot/internal/true-heading-error-deg</prop>
  </input>
  <reference>
    <value>0.0</value>
  </reference>
  <output>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </output>
  <config>
    <Kp>-2.0</Kp>        <!-- proportional gain -->
    <Ki>0.0</Ki>         <!-- integral gain -->
    <u_min>-30.0</u_min> <!-- minimum output clamp -->
    <u_max>30.0</u_max>  <!-- maximum output clamp -->
  </config>
</pi-simple-controller>

<!-- Stage #2 drives the ailerons to achieve the desired roll deg. -->
<pid-controller>
  <name>True Heading Hold (DG based) Stage 2</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>true-heading-hold</value>
    <honor-passive>true</honor-passive>
  </enable>
  <input>
    <prop>/orientation/roll-deg</prop>
  </input>
  <reference>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </reference>
  <output>
    <prop>/controls/flight/aileron</prop>
  </output>
  <config>
    <Kp>0.5</Kp>        <!-- proportional gain -->
    <beta>1.0</beta>    <!-- input value weighing factor -->
    <alpha>0.1</alpha>  <!-- low pass filter weighing factor -->
    <gamma>0.0</gamma>  <!-- input value weighing factor for -->
                        <!-- unfiltered derivative error -->
    <Ti>10.0</Ti>       <!-- integrator time -->
    <Td>0.00001</Td>    <!-- derivator time -->
    <u_min>-1.0</u_min> <!-- minimum output clamp -->
    <u_max>1.0</u_max>  <!-- maximum output clamp -->
  </config>
</pid-controller>


<!-- Nav1 hold.  2 stage cascade controller. -->

<!-- Stage #1 sets target roll based on nav1-heading-error-deg. -->
<pid-controller>
  <name>Nav1 Hold Stage 1</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>nav1-hold</value>
  </enable>
  <input>
    <prop>/autopilot/internal/nav1-heading-error-deg</prop>
  </input>
  <reference>
    <value>0.0</value>
  </reference>
  <output>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </output>
  <config>
    <Kp>-1.3</Kp>        <!-- proportional gain -->
    <beta>1.0</beta>     <!-- input value weighing factor -->
    <alpha>0.1</alpha>   <!-- low pass filter weighing factor -->
    <gamma>0.0</gamma>   <!-- input value weighing factor for -->
                         <!-- unfiltered derivative error -->
    <Ti>40</Ti>          <!-- integrator time -->
    <Td>0.00001</Td>     <!-- derivator time -->
    <u_min>-30.0</u_min> <!-- minimum output clamp -->
    <u_max>30.0</u_max>  <!-- maximum output clamp -->
  </config>
</pid-controller>

<!-- Stage #2 drives the ailerons to achieve the desired roll deg. -->
<pid-controller>
  <name>Nav1 Hold Stage 2</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/heading</prop>
    <value>nav1-hold</value>
    <honor-passive>true</honor-passive>
  </enable>
  <input>
    <prop>/orientation/roll-deg</prop>
  </input>
  <reference>
    <prop>/autopilot/internal/target-roll-deg</prop>
  </reference>
  <output>
    <prop>/controls/flight/aileron</prop>
  </output>
  <config>
    <Kp>0.2</Kp>        <!-- proportional gain -->
    <beta>1.0</beta>    <!-- input value weighing factor -->
    <alpha>0.1</alpha>  <!-- low pass filter weighing factor -->
    <gamma>0.0</gamma>  <!-- input value weighing factor for -->
                        <!-- unfiltered derivative error -->
    <Ti>10.0</Ti>       <!-- integrator time -->
    <Td>0.00001</Td>    <!-- derivator time -->
    <u_min>-1.0</u_min> <!-- minimum output clamp -->
    <u_max>1.0</u_max>  <!-- maximum output clamp -->
  </config>
</pid-controller>


<!-- ================================ -->
<!-- ======= Pitch Axis Modes ======= -->
<!-- ================================ -->

<!-- Simple pitch hold -->
<pid-controller>
<name>Pitch hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>pitch-hold</value>
</enable>
<input>
<prop>/orientation/pitch-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/target-pitch-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.15</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>5.0</Ti>
<!-- integrator time -->
<Td>0.1</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple pitch hold with yoke -->
<pid-controller>
<name>Pitch hold w/ yoke</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>pitch-hold-yoke</value>
</enable>
<input>
<prop>/orientation/pitch-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/target-pitch-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator</prop>
</output>
<config>
<Kp>-0.05</Kp>
<!-- proportional gain (was 0.05)-->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>.5</Ti>
<!-- integrator time (was 1.0) -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple angle of attack hold -->
<pid-controller>
<name>AOA hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>aoa-hold</value>
</enable>
<input>
<prop>/orientation/alpha-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/target-aoa-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.05</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>0.5</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
Altitude hold.  2 stage cascade controller.
Stage #1 sets target rate of climb based on diff between current alt
and target altitude.
-->
<pi-simple-controller>
  <name>Altitude Hold (Altimeter based) Stage 1</name>
  <debug>false</debug>
  <enable>
    <prop>/autopilot/locks/altitude</prop>
    <value>altitude-hold</value>
  </enable>
  <input>
    <prop>/position/altitude-ft</prop>
  </input>
  <reference>
    <prop>/autopilot/settings/target-altitude-ft</prop>
  </reference>
  <output>
    <prop>/autopilot/internal/target-climb-rate-fps</prop>
  </output>
  <config>
    <Kp>0.3</Kp>
    <!-- proportional gain -->
    <Ki>0.0</Ki>
    <u_min>-33.3</u_min>
    <!-- minimum output clamp -->
    <u_max>33.3</u_max>
    <!-- maximum output clamp -->
  </config>
</pi-simple-controller>

<!-- Stage #2 drives the elevator-trim to achieve the desired climb rate. -->
<pid-controller>
<name>Altitude Hold (Altimeter based) Stage 2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>altitude-hold</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.002</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
AGL hold.  2 stage cascade controller.
Stage #1 sets target rate of climb based on diff between current agl
and target agl.
-->
<pid-controller>
<name>AGL Hold (Altimeter based) Stage 1</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>agl-hold</value>
</enable>
<input>
<prop>/position/altitude-agl-ft</prop>
</input>
<reference>
<prop>/autopilot/settings/target-agl-ft</prop>
</reference>
<output>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</output>
<config>
<Kp>0.3</Kp>
<!-- proportional gain -->
<Ki>0.0</Ki>
<beta>1.0</beta>
<!-- input value weighing factor -->
<u_min>-33.33</u_min>
<!-- minimum output clamp -->
<u_max>33.33</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Stage #2 drives the elevator-trim to achieve the desired climb rate. -->
<pid-controller>
<name>Altitude Hold (Altimeter based) Stage 2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>afl-hold</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.001</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Glideslope hold. -->


<pid-controller>
<name>Glideslope Hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>gs1-hold</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/instrumentation/nav[0]gs-rate-of-climb</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.004</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-.68</u_min>
<!-- minimum output clamp -->
<u_max>.68</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
==============
Velocity Modes
==============
-->
<!-- Simple Auto throttle -->
<pid-controller>
<name>Auto Throttle</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/speed</prop>
<value>speed-with-throttle</value>
</enable>
<input>
<prop>/velocities/airspeed-kt</prop>
</input>
<reference>
<prop>/autopilot/settings/target-speed-kt</prop>
</reference>
<output>
<prop>/controls/engines/engine[0]/throttle</prop>
<prop>/controls/engines/engine[1]/throttle</prop>
<prop>/controls/engines/engine[2]/throttle</prop>
<prop>/controls/engines/engine[3]/throttle</prop>
<prop>/controls/engines/engine[4]/throttle</prop>
<prop>/controls/engines/engine[5]/throttle</prop>
</output>
<config>
<Kp>0.1</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.001</Td>
<!-- derivator time -->
<u_min>0.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Hold speed by varying pitch (Two stage cascading controller) -->
<pid-controller>
<name>Speed hold (vary pitch) Stage #1</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/speed</prop>
<value>speed-with-pitch</value>
</enable>
<input>
<prop>/velocities/airspeed-kt</prop>
</input>
<reference>
<prop>/autopilot/settings/target-speed-kt</prop>
</reference>
<output>
<prop>/autopilot/settings/target-pitch-deg</prop>
</output>
<config>
<Kp>.05</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>0.2</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-15.0</u_min><!-- minimum output clamp -->
<u_max>15.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<pid-controller>
<name>Speed hold (vary pitch) Stage #2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/speed</prop>
<value>speed-with-pitch-trim</value>
</enable>
<input>
<prop>/orientation/pitch-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/target-pitch-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.05</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>1.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- ==========================================================-->
<!-- Custom Controllers -->
<!-- ==========================================================-->
<!-- Modified pitch hold for take-offs -->
<pid-controller>
<name>T-O Pitch hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>take-off</value>
</enable>
<input>
<prop>/orientation/pitch-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/take-off-pitch-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.8</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>8.0</Ti>
<!-- integrator time -->
<Td>0.1</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Modified pitch hold for initial climb-out -->
<pid-controller>
<name>Climb Out Pitch hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>climb-out</value>
</enable>
<input>
<prop>/orientation/pitch-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/climb-out-pitch-deg</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.06</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.01</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Auto throttle (Mach Hold)-->
<pid-controller>
<name>Auto Throttle (Mach Hold)</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/speed</prop>
<value>mach-with-throttle</value>
</enable>
<input>
<prop>/velocities/mach</prop>
</input>
<reference>
<prop>/autopilot/settings/target-mach</prop>
</reference>
<output>
<prop>/controls/engines/engine[0]/throttle</prop>
<prop>/controls/engines/engine[1]/throttle</prop>
<prop>/controls/engines/engine[2]/throttle</prop>
<prop>/controls/engines/engine[3]/throttle</prop>
<prop>/controls/engines/engine[4]/throttle</prop>
<prop>/controls/engines/engine[5]/throttle</prop>
</output>
<config>
<Kp>20.0</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>0.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
Mach Climb Hold.
Two stage controller based on modified Altitude hold.
Stage #1 sets target rate of climb based on diff between
current mach and target mach.
-->
<pid-controller>
<name>Mach Lock Climb Stage 1</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>mach-climb</value>
</enable>
<input>
<prop>/autopilot/settings/target-mach</prop>
</input>
<reference>
<prop>/velocities/mach</prop>
</reference>
<output>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</output>
<config>
<Kp>1600.0</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.01</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>40.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>50.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Stage #2 drives the elevator-trim to achieve the desired climb rate. -->
<pid-controller>
<name>Mach lock Climb Stage 2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>mach-climb</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.008</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
Modified AGL hold for autopilot landing - 2 stage cascade controller.
Stage #1 sets target rate of climb based on diff between current agl
and target (zero) agl
-->
<pid-controller>
<name>Auto Landing Stage 1</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>Touch Down</value>
</enable>
<input>
<prop>/position/altitude-agl-ft</prop>
</input>
<reference>
<value>0.0</value>
</reference>
<output>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</output>
<config>
<Kp>0.051</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.001</Td>
<!-- derivator time -->
<u_min>-12.0</u_min>
<!-- minimum output clamp -->
<u_max>-0.10</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Stage #2 drives the elevator-trim to achieve the desired climb rate. -->
<pid-controller>
<name>Auto Landing Stage 2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>Touch Down</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/autopilot/internal/target-climb-rate-fps</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.02</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>2.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple Ground Roll Rudder Heading Hold -->
<pid-controller>
<name>Ground Roll Rudder hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/rudder-control</prop>
<value>rudder-hold</value>
</enable>
<input>
<prop>/orientation/heading-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/ground-roll-heading-deg</prop>
</reference>
<output>
<prop>/controls/flight/rudder</prop>
</output>
<config>
<Kp>0.5</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>5.0</Ti>
<!-- integrator time -->
<Td>0.1</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple AoA-by-speed Hold -->
<pid-controller>
<name>AoA-by-speed Hold</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/AoA-lock</prop>
<value>Engaged</value>
</enable>
<input>
<prop>/orientation/alpha-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/AoA-deg</prop>
</reference>
<output>
<prop>/autopilot/settings/target-speed-kt</prop>
</output>
<config>
<Kp>-3.0</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.001</Td>
<!-- derivator time -->
<u_min>90.0</u_min>
<!-- minimum output clamp -->
<u_max>160.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple Flap Control -->
<pid-controller>
<name>Simple Flap Control</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/auto-flap-control</prop>
<value>Engaged</value>
</enable>
<input>
<prop>/orientation/alpha-deg</prop>
</input>
<reference>
<prop>/autopilot/settings/auto-flap-target-deg</prop>
</reference>
<output>
<prop>/controls/flight/flaps</prop>
</output>
<config>
<Kp>-0.1</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>10.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>0</u_min>
<!-- minimum output clamp -->
<u_max>1</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!--
Nav1 hold - Final approach.  2 stage cascade controller.
Stage #1 sets target roll based on heading-needle-deflection.
-->
<pid-controller>
<name>Nav1 Hold Stage 1</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/heading</prop>
<value>nav1-hold-fa</value>
</enable>
<input>
<prop>/instrumentation/nav[0]/heading-needle-deflection</prop>
</input>
<reference>
<value>0.0</value>
</reference>
<output>
<prop>/autopilot/internal/target-roll-deg</prop>
</output>
<config>
<Kp>-10.0</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>60</Ti>
<!-- integrator time -->
<Td>4.0</Td>
<!-- derivator time -->
<u_min>-6.0</u_min>
<!-- minimum output clamp -->
<u_max>6.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Stage #2 drives the ailerons to achieve the desired roll deg. -->
<pid-controller>
<name>Nav1 Hold Stage 2</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/heading</prop>
<value>nav1-hold-fa</value>
</enable>
<input>
<prop>/orientation/roll-deg</prop>
</input>
<reference>
<prop>/autopilot/internal/target-roll-deg</prop>
</reference>
<output>
<prop>/controls/flight/aileron</prop>
</output>
<config>
<Kp>0.6</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>4.0</Ti>
<!-- integrator time -->
<Td>0.00001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>
<!-- Simple VFPS hold (low-speed) -->
<pid-controller>
<name>VFPS Hold (low-speed)</name>
<debug>false</debug>
<enable>
<prop>/autopilot/locks/altitude</prop>
<value>vfps-hold-ls</value>
</enable>
<input>
<prop>/velocities/vertical-speed-fps</prop>
</input>
<reference>
<prop>/autopilot/settings/target-vfps</prop>
</reference>
<output>
<prop>/controls/flight/elevator-trim</prop>
</output>
<config>
<Kp>-0.018</Kp>
<!-- proportional gain -->
<beta>1.0</beta>
<!-- input value weighing factor -->
<alpha>0.1</alpha>
<!-- low pass filter weighing factor -->
<gamma>0.0</gamma>
<!-- input value weighing factor for -->
<!-- unfiltered derivative error -->
<Ti>6.0</Ti>
<!-- integrator time -->
<Td>0.001</Td>
<!-- derivator time -->
<u_min>-1.0</u_min>
<!-- minimum output clamp -->
<u_max>1.0</u_max>
<!-- maximum output clamp -->
</config>
</pid-controller>

</PropertyList>

