<?xml version="1.0"?>
<!--
    Usable with FlightGear
    Property of Gerard Robin
    Copyright License:  GPL
-->
<PropertyList>

        <title>SR71-BackBird</title>
        <key>
                <name>}</name>
                <desc>toggle Electric Master Switch On/Off</desc>
        </key>
        <key>
                <name>Space  or "s" (if your keyboard.xml has been updated from CVS) </name>
                <desc>Starter</desc>
        </key>

        <key>
                <name>{</name>
                <desc>toggle Cutoff ON/OFF</desc>
        </key>
        <key>
                <name>d</name>
                <desc>Toggle canopy</desc>
        </key>
        <key>
                <name>F</name>
                <desc>Toggle refuel  on/off</desc>
        </key>
        <!--<key>
                <name>Ctrl-H</name>
                <desc>Toggle Unlock/Lock Autopilot </desc>
        </key>-->
        <key>
                <name>Ctrl-A</name>
                <desc>Toggle Unlock/Lock Autopilot on the current Altitude</desc>
        </key>
        <key>
                <name>Ctrl-b</name>
                <desc>Prepare braking chute deployement, open the doors</desc>
        </key>
        <key>
                <name>j</name>
                <desc>Reload Braking Chute, and close the doors</desc>
        </key>
        <text>
          First Contact with Blackbird
          Now you are sitting in the Pilot cockpit
          On the Forward Cockpit if Blackbird   SR71-A
          With view "7" you can see the RSO cockpit (not yet with equipemnts)
          On the Rear Cockpit if Blackbird   SR71-B  training
          With view "7" you can see the Pilot Student cockpit
          The Electric Master is OFF
          The Engines is "cut off" ON
          The canopy are "open"
          The Parking Brake is ON

          ====Start Routine==========
          Electric Master Switch On => key "}"
          Get the external Starter ressources
          (depress "space" or "s" if you have just updated you CVS data keyboard.xml)
          The engine will spin up to a maximum of about %25 N2 (%5.2 N1)
          This simulates the action of the external starter.
          After reaching %15 N2,  Cutoff to False  => key "{"
            wait for the EP Ratio needle close to 1.1
          Don't forget to close the canopy key => "d"
          Parking brake Off
          then push the throttle to  take off

          ====To get 85000 feets=======
          This is the procedure for the model, not for the real one (smile)
          After take Off and Landing gear UP, set the trottle to maximum and
          set the Autopilot "Pitch Hold" to 10
          You can notice the Aircraft climbing , and the speed increasing  to 1.1 Mach
          When you are at 29000 feet altitude stop to climb by
          setting the Autopilot "Altitude Hold" to 30000
          The speed will increase to 3.0 Mach
          Again set the Autopilot "Pitch Hold" to 10
          The aircraft will climb, when at 83000 feets
          set the Autopilot "Altitude Hold"  to 85000

          ====Refueling============
          With key "F"
          On gound refueling, if Airspeed less than 20 kts
          Does not need Probe, the probe is not raised
          Air refueling if Airspeed more than 200 kts and Agl more  than 300 feet
          Probe is first automatically raised
          for your facility it does not need refuel contact with Tanker
          however, the air refueling function  is automatically activated if you get the contact with the tanker


          ====Braking Chute==========
          the braking chute will be automaticlly deployed
          When the following conditions are all true

          Brake Chute doors are openeded  => key "Ctrl-b"
          Airspeed less than 200 kts
          Agl less than 20 feet
          Throttle position less than 0.1

          the braking chute will be released, untied
          When
          Airspeed less than 50 kts
          REMEMBER       it can be used only once
          If you want it again you must reload it =>  key "j"

          ====Radar================
          That Radar is the last version ("Vivian" Radar )
           you can choose the range by clicking on the switch
           =>mouse button 1 to decrease =>mouse button 0 to increase

          ====Tacan================
          The Tacan instrument is situated or the left side of the cockpit
          That instrument is fully operationnal, look at the hotspot to enter the right values
          ====Autopilot==============
          The autopilot can be ON/OFF with Altitude and Heading
           with key => "Ctrl A"  (toggle ON/OF) for the current Altitude
        <!--  with key => "Ctrl H"  (toggle ON/OF) for the choosen bug heading on your HSI instrument    -->

        </text>

</PropertyList>