/*****************************/
/***** English version *******/
/*****************************/

Kicad binaries exists for Linux and Windows (XP, 2000)
Files (schematic, boards, libraries) created on both systems are totally compatibles.

Used language:
Doc files are in french, but kicad user interface is internationalized:
User interface is in English for most countries.
User interface is in French **only** if you run kicad from a french version of Linux or Windows.
It is easy to add a new translation with poedit.
Kicad can use this translation without any change.
(poedit is used to create the french translation).
See http://poedit.sourceforge.net.
Contact me for more details.

Installation form archives:
(both have binary file for Linux and Windows XP and 2000 (not Window 98) )
kicad.zip
or
kicad.tgz

Untar or unzip kicad
this create the kicad tree in the current directory.

**Under Windows:
Goto C:\ or D:\ (or other prefered directory).
Examples are for an install on C:\.
Unzip kicad.zip
You must have created c:\kicad.
Windows executables are in c:\kicad\winexe.
The main program is kicad.exe and from it you can run other programs
(schematic, pcb, utilities: cvpcb, gerbview and other) )
I suggest you create a shortcut to c:\kicad\winexe\kicad.exe


** Under Linux:
You do must have libc.so.6 (do not work with libc.so.5)
You must be "root".
goto /usr/local
Untar kicad.tgz : tar zxvf kicad.tgz (ou unzip kicad.zip)
(It is possible to unzip kicad.zip: unzip kicad.zip,
and goto /usr/local/kicad/linux and run chmod 755 *)
The main program is /usr/local/kicad/linux/kicad
If you use KDE, users can copy the shortcut /usr/local/kicad/linux/kicad.desktop
in <user home directory>/Desktop and use it to run kicad.

3D modeler wings3D:
(Usefull only if you plan to create 3D shapes for Printed board modules)
Archive and doc files (Linux and windows ) are in ../kicad/wing3d
goto www.wings3d.org to have more details.
Pcbnew use the exported files in wrml (.wrl) format from wings3d (not the native .wings format).

Documentation:
Currenty only in french.
"On line" in html format.
source files (200 sheets) are in OpenOffice (www.openoffice.org) format.
Can be read, printed and/or modified with OpenOffice.
See files in kicad/help/doc_src/*

Kicad tree:
kicad/winexe: windows (XP et 2000 compatible) binaries.
kicad/linux: linux  binaries (Mandrake 9.2 and 10.0 tested,
	probably work fine for distributions who have an recent libc)
kicad/library: libraries for schematic
kicad/library/doc: documentation files for schematic components (.pdf)
	(readable from schematic if you have acrobat ou Xpdf)
kicad/modules: module libraries for printed boards.
	files *.mod are the libraries,
	and files *.brd are printed board you can see with pcbnew
	files *.brd show the existing modules (and 3D shapes) in libraries. 
kicad/modules/packages3d: many 3D shapes (.wrl et .wings format) for existing modules

kicad/demos: Usefull...
kicad/internat: dictionnaires des langues (actuellement anglais->francais) pour les menus
kicad/help: On line help (in french)
kicad/help/doc_src: Documentation (in french) (source doc, 200 sheets) under OpenOffice.

Warning:
Do not change the kicad tree, or the location of binary files,
or kicad will **not** be able to found other kicad files (configuration, libraries...)


/*******************************/
/***** version Francaise *******/
/*******************************/

Les executable kicad existent pour Linux et Windows (XP, 2000)
Les fichiers crees (Schematique, circuits imprimes, librairies) sous ces 2 systemes sont
totalement compatibles.

Installation a partir des archives
(toutes les 2 contiennent **tous** les executables):
kicad.zip
ou
kicad.tgz (s'il est disponible)

Le decompactage cree le repertoire kicad (et ses sous repertoires) a partir
du repertoire courant.

**Sous Windows:
se placer dans C:\ (ou D:\ ou tout disque et repertoire de son choix)
On supposera ici que l'on s'est placé dans c:\
Decompacter kicad.zip
Créer un raccourci vers c:\kicad\winexe\kicad.exe
On pourra alors lancer le gestionnaire de projets kicad.exe

Sous Linux
On se placera de préférence en /usr/local
Il faudra sans doute aussi etre "root"
Decompacter kicad.tgz ou kicad.zip
  - kicad.tgz: faire tar zxvf <chemin de kicad.tgz>/kicad.tgz
  - kicad.zip (unzip <chemin de kicad.tgz>/kicad.zip). Il faudra alors dans ce
    cas rendre executable kicad, cvpcb, eeschema, gerbview et pcbnew:
	se placer dans /usr/local/kicad/linux et faire la commande chmod 755 nom_fichier
	pour ces 5 fichiers.
On lancera kicad par /usr/local/kicad/linux/kicad
Sous KDE on pourra copier /usr/local/kicad/linux/kicad.desktop sur le bureau
de KDE comme raccourci.

Installation du modeleur 3D wings3D pour créer les formes 3D des modules du PCB:
Il est fourni dans ..kicad/wings3d pour Windows et Linux.
Se reporter au site du créateur pour tous détails (www.wings3d.org)
Se reporter aussi a la doc de pcbnew pour la génération des fichiers 3d

Documentation:
L'impression de la documentation (environ 200 pages) peut se faire
sous OpenOffice (www.openoffice.org) (magnifique logiciel libre de traitement de texte).

Principaux repertoires de Kicad:
kicad/winexe: executables sous windows (teste sous XP et 2000)
kicad/linux: executables sous linux (testes sous Mandrake 9.2 et 10.0)
kicad/library: fichiers libraires de composants schematiques
kicad/library/doc: fichiers documentation des composants schematiques (.pdf)
	(accessibles directement de la schematique si l'on a installé acrobat ou Xpdf)
kicad/modules: fichiers de composants (modules) pour le circuit imprimé
kicad/modules/packages3d: fichiers de formes 3D des modules

kicad/demos: C'est toujours utile...
kicad/internat: dictionnaires des langues (actuellement anglais->francais) pour les menus
kicad/help: fichiers d'aides en ligne
kicad/help/doc_src: fichiers d'aides (doc source, 200 pages) sous OpenOffice,
	a lire avant de se plaindre.


Complements:
-En cas de difficulté:
Un problème peut surgir pour kicad lors de la recherche des fichiers utiles
comme fichiers de config, librairies, dictionnaire anglais->français, docs...
Sous Windows:
	La recherche se fait là ou sont lus les executables.
	Il ne faut donc pas recopier les executables ailleurs que là ou ils sont.
	Toutefois, si cela ne marche pas, kicad cherche le repertoire c:\kicad
Sous linux:
	La recherche se fait sur /usr/local/kicad (installation conseillée),
	ou dans le chemin des executables si /usr/local/kicad n'est pas trouvé.

Uniquement en cas d'installation non standard (et en cas de difficulté),
definir la variable d'environnement KICAD = <chemin de kicad>
ex: KICAD=/usr/local/cao/kicad
