In embedded applications on low-powered processors, performance is a big
issue. Using either the KCM or Comba methods as described here can increase
speeds 4-fold.

To use the super-fast KCM (for 2048-bit RSA 1024-bit DH and DSS) and Comba 
(for 1024 bit RSA and GF(p) Elliptic curves) methods you will need to create 
the file mrkcm.c or the file mrcomba.c for inclusion in the MIRACL library. 
This is done by inserting 'macros' from a ?.mcs file into the template files 
mrkcm.tpl, or mrcomba.tpl. This is done automatically using the MEX utility.

A c.mcs file is supplied, which contains C macros. Also c1.mcs which uses
an alternate approach. See also cs.mcs (read the comments at the top).
However the best performance is usually achieved by 
using assembly language macros. This requires your compiler to support in-line 
assembly. For example the file ms86.mcs inserts Pentium assembly language 
macros for use with Microsoft or Borland compilers. The file gcc386.mcs does 
the same for the gcc compiler. If your PC supports SSE2 extensions, for 
example if it is a Pentium 4, then instead use either sse2.mcs or gccsse2.mcs 
(see sse2.txt). The file arm.mcs does the same for the popular 32-bit ARM 
processor. Other .mcs files for other processors/compilers may be available. 
See makemcs.txt for instructions for creating your own.

New! The files c.mcs and arm.mcs now allow "interleaved" multiplication steps 
to facilitate improved processor scheduling - see makemcs.txt.

The macro expansion is carried out automatically by the supplied program 
MEX.C. You must compile and run this program. If you use the config.c 
utility it will advise you on the parameters to use. Note that although 
config.c should be compiled and run on the target processor, mex.c can be 
compiled and run on any workstation.

For example

c:>mex 6 ms86 mrcomba

creates a file mrcomba.c from mrcomba.tpl and ms86.mcs. The Comba method will
then be optimised for a modulus of 6*32 = 192 bits on a Pentium computer. 
Typically this might be used for an implementation of elliptic curves over 
GF(p) for p a 192 bit prime. Note that the code generated in mrcomba.c or 
mrkcm.c may benefit to a small extent from some manual post-optimisation. 
Re-ordering instructions may help for certain processors.

c:>mex 16 ms86 mrkcm

creates a file mrkcm.c from mrkcm.tpl and ms86.mcs. The KCM method will then 
be optimised for moduli of sizes 512, 1024, 2048 bits etc. Typically this 
might be used for a fast implementation of RSA, DSS or Diffie-Hellman. 

For the Comba method only it is possible to implement special modular 
reduction methods for a modulus p of a particular form. This requires 
manual implementation and editing of the file mrcomba.tpl. There you will
find example code for the cases of p=2^192-2^64-1 and p=2#224-2#96+1. To make 
use of this feature MR_SPECIAL must be defined in mirdef.h. As always it is 
best to use config.c, which guides you through all of this. 

You will find it valuable to run through this whole process on a standard PC
using perhaps the Microsoft C/C++ compiler, just to get familiar with the 
config.c and mex.c utilities.

If you are embarking on an embedded project using a processor for which a 
.mcs file does not exist, you will have to write your own, or be content with 
the C macros. Note that this approach is likely to be optimal only on 
processors that support an unsigned multiply instruction. 
This is probably the case with the majority of embedded processors (e.g. ARM, 
68000 variants etc). It is also important that the compiler support inline 
assembly, via something like

asm("  ");

or

__asm

{
}

constructs in C. However other approaches are possible, for example using C 
"intrinsics" works well for the itanium - see itanium.mcs

To write your own .mcs file, use c.mcs or arm.mcs as models. For more 
background read the article ftp.computing.dcu.ie/pub/crypto/timings.doc

The macro-expansion mechanism has been designed to make it as easy as 
possible for the developer to write optimal code for best performance.
See makemcs.txt


