AtariMax 1M Bit Programmable Cart

AtariMax 1 Mega Bit Programmable Cart

To my knowledge this was the first user programmable cartridge!

The First way to Start off the programmable process was to make or obtain an ATR file with the cart image within it. Then Mount the cart.atr file as drive one with your APE software. Insert the target 1 mb AtariMax Cartridge into your Atari 8-bit computer that is equipped with a SIO2PC with your ATR image set as Drive 1. Reboot your computer and follow the instructions.

The second way is by far the best way to program on of these carts. Using a MaxFlash device. The MaxFlash Hooks up to your IBM Clones USB port and can read ANY ATARI 8-Bit Cartridge and can write to AtariMax Cartridges This by far is the fastest way to program your AtariMax Cartridges

Their are two things you need to remember when using the AtariMax Cartridges. They have their own banking schemes that may be different than the original Cart you copied. The AtariMax Cartridges were not designed to be stacked like the ICD SDX, Express, Diamond, Multiplexer, and R-Time 8.

About ILS - Contact us - Report Web Issues