Internal Multi OS Project Page

How to Build your own Quad OS

Part need for this project:

1 High quality 28 pin IC sockets

Few feet of 22 gauge wire

1 27512 E-Prom

2 Single pole single throw switch

2 1 kOhm 1/8watt resister

Desolder with a devack Soldering tool the OS chip in your Atari. With a 15 watt Soldering iron solder in your socket onto your mother board.

First thing you need to do is pick 4 Atari OS images. Then burn the OS images you want into the 4 16k banks. Bend out pins 1 & 27. (Make sure you always put the Standard OS into one of the banks for compatibility)

Solder one leg of one resister to pin 1. Solder 1 wire to pin 1 and solder the other end of the wire to one leg of your switch.

Solder one leg of one resister to pin 27. Solder 1 wire to pin 27 and solder the other end of the wire to one leg of your switch.

bend each leg of the other end of both resister to pin 28 of your 27512 E-Prom. Make sure to leave enough of pin 28 to be insert into your socket.

Now solder 1 wire to pin 14 (ground) and the other end to one of the unsolder legs of the switch. Then run a jumper from the ground wire you just connected to the other switch leg that has not be soldered.

Now your done! It should look like this!.

While there are many OS upgrades this is a very stable one. This upgrade will not work with a Ultra Speed Plus OS Image. I use this very Rom In my Multiplexer Master Machine. I have a Standard OS, Omnimon, Turboss, and a Fix XL OS.

Your Standard Atari OS is a 16k Rom Image. The 27512 E-Prom is 4 times as large as the rom you took out of your machine.

27128 Rom = $0000-$3FFF mapped into $C000-$FFFF

27512 E-Prom = $0000-$FFFF is broke into 4 banks that map into your Atari at $C000-$FFFF

Bank1 = $0000-$3FFF

Bank2 = $4000-$7FFF

Bank3 = $8000-$BFFF

Bank 4 = $C000-$FFFF

You can use this same circuit to create a OSS Super Cart with all the OSS language Roms. Here is a picture of an OSS Super Cart that uses 1 27128 E-Prom. Not all of the OSS Super Cart use a single Chip. Fact is the Vast number of OSS Super Carts use 2 2764 Roms for their carts. But if you have a OSS Cart that is single chip here is a rom image to build an OSS Super Cart with Mac/65, Basic XL, Basic XE, and Action.

My QUAD OS with 256 byte Phantom SRam

This is a Multi OS Board. It uses a 27512 e-prom which give you 4 OS. It also has a page of S-Ram mapped into d7xx so that CSS Ultra-Speed Plus OS can function. I have not cad this yet but as soon as I do I will post it here.

Here are the Operating Systems Documentation I use the Most and their documentation. Their is E-Prom Images in my download section of this web site

Ominmon

Ominview

Multiplexer

Ultra-Speed Plus

Turboss

Once again these are modification I own and have. If you have a mod I do not have please e-mail me I would Like to here about it.

About ILS - Contact us - Report Web Issues