8-Bit Ram-Disk Upgrades Page

Home | Review Menu | 320kxe | 576kxe | 1088kxe | 1088kxe 2

11/05/2012

On the tabs have documents that I have used to upgrade Atari 130xe

10/30/2012

This is my Design of a battery backed R amdisk.

I have been using this ramdisk for years. It uses normal pins on the pia so most all ramdisk drivers will

Work. The real trick is to have a ramdisk driver that does not auto format the ramdisk. The ramdisk

Driver in RealDos does not auto format. SpartaDos X does not auto format ether.

About ILS - Contact us - Report Web Issues