# 5.25" Power

Used for harddisks & 5.25" peripherals.
Name according to the ATX standard: Peripheral Connector.

(at the powersupply cable)
(at the peripheral)

UNKNOWN CONNECTOR at the powersupply cable.
UNKNOWN CONNECTOR at the peripheral.

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | +12V |  | Yellow | +12 VDC
2 | GND |  | Black | +12 V Ground (Same as +5 V Ground)
3 | GND |  | Black | +5 V Ground
4 | +5V |  | Red | +5 VDC

Recommended wiresize according to the ATX standard: 18 AWG
At cables: AMP 1-480424-0 or Molex 8981-04P
At peripherals: AMP 61314-1

Contributor: | Joakim Ögren, Eric Sprigg, Sven Gunnar Bilen, Scott Lindenthaler

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13