# 64NET

(To C64).
(To PC).

DZM 12 DREH to the C64 UserPort.
25 PIN D-SUB MALE to the PC

| C64 | Dir | PC |
--- | --- | --- | --- | ---
GND | A |  | 25 | GND
PB0 | C |  | 10 | /ACK
PB1 | D |  | 11 | BUSY
PB2 | E |  | 12 | PE
PB3 | F |  | 5 | D3
PB4 | H |  | 6 | D4
PB5 | J |  | 7 | D5
PB6 | K |  | 8 | D6
PB7 | L |  | 9 | D7

Contributor: | Joakim Ögren

Source: | 64NET v1.82.58 documentation by Paul Gardner-Stephen

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10