# DIN Audio

(at the peripheral)
(at the cable)

5 PIN DIN 180° (DIN41524) FEMALE at the peripheral.
5 PIN DIN 180° (DIN41524) MALE at the cable.

Peripheral | Connected | In L | In R | Out L | Out R | Ground
--- | --- | --- | --- | --- | --- | ---
Amplifier | Pickup, tuner | 3 | 5 |  |  | 2
Amplifier | Taperecorder | 3 | 5 | 1 | 4 | 2
Tuner | Amplifier |  |  | 3 | 5 | 2
Tuner | Taperecorder |  |  | 1 | 4 | 2
Recordplayer | Amplifier |  |  | 3 | 5 | 2
Taperecorder | Amplifier | 1 | 4 | 3 | 5 | 2
Taperecorder | Receiver | 1 | 4 | 3 | 5 | 2
Taperecorder | Microphone | 1 | 4 |  |  | 2

Contributor: | Joakim Ögren

Source: | ELFA's catalog Nr 44

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10