# C64 Centronics Printer

Requires a cartridge with Centronics support (TFCIII or ActionReplay.)

(to the C64).
(to the Printer)

DZM 12 DREH to the C64 UserPort.
36 PIN CENTRONICS MALE to the Printer.

| C64 | Dir | Printer |
--- | --- | --- | --- | ---
GND | 1,12,A,N |  | 19-30,33 | Ground
FLAG2 | B |  | 10 | Acknowledge
PB0 | C |  | 2 | Data 0
PB1 | D |  | 3 | Data 1
PB2 | E |  | 4 | Data 2
PB3 | F |  | 5 | Data 3
PB4 | H |  | 6 | Data 4
PB5 | J |  | 7 | Data 5
PB6 | K |  | 8 | Data 6
PB7 | L |  | 9 | Data 7
PA2 | M |  | 1 | Strobe
GND | 3 |  | 31 | Initialize Printer

Contributor: | Joakim Ögren

Source: | CBM Memorial Page Pinouts - pinout by Roy Kannady

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10