# C16/C116/+4 Joystick

Available on the Commodore C16, C116 and +4 computers.

(at the computer)

8 PIN MINI-DIN FEMALE at the computer.

## Joystick 1

Pin | Name | Dir | Comment
--- | --- | --- | ---
1 | JOYA0 |  |
2 | JOYA1 |  |
3 | JOYA2 |  |
4 | JOYA3 |  |
5 | +5VDC |  |
6 | BUTTON A | ? |
7 | GND |  |
8 | COMMON A ? | ? | Is connected to DATA2 thru a buffer.

## Joystick 2

Pin | Name | Dir | Comment
--- | --- | --- | ---
1 | JOYB0 |  |
2 | JOYB1 |  |
3 | JOYB2 |  |
4 | JOYB3 |  |
5 | +5VDC |  |
6 | BUTTON B | ? |
7 | GND |  |
8 | COMMON B ? | ? | Is connected to DATA1 thru a buffer.

Note: Direction is Computer relative Device.

Contributor: | Joakim Ögren, Arwin Vosselman
Source: | SAMS Computerfacts CC8 Commodore 16.
Copyright © The Hardware Book Team 1996-2004. May be copied and redistributed, partially or in whole, as appropriate. Document last modified: 2002-01-10