# WTX 12V CPU (P3)

8 PIN MOLEX 39-29-9082 CONNECTOR at the Motherboard
8 PIN MOLEX 39-01-2080 CONNECTOR at the cable

Pin | Name |  | Color | Description | AWG
--- | --- | --- | --- | --- | ---
1 | 12Vdig |  | White | +12 VDC (Digital) | 18
2 | 12Vdig |  | White | +12 VDC (Digital) | 18
3 | 12Vdig |  | White | +12 VDC (Digital) | 18
4 | 12Vdigsen |  |  | Sense +12 VDC (Digital) (Optional?) |
5 | com |  | Black | Ground | 18
6 | com |  | Black | Ground | 18
7 | com |  | Black | Ground | 18
8 | 12Vdigsenrtn |  |  | Ground Sense +12 VDC (Digital) (Optional?) |

Contributor: | Joakim Ögren

Source: | WTX Power Supply Design Guidelines at WTX Website

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10