# C16/C116/+4 Audio/Video

Available on Commodore C16/C116/+4 computers.

(at the Computer)

8 PIN DIN (DIN45326) FEMALE at the Computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | LUM |  | Luminance (monochrome video)
2 | GND |  | Ground
3 | AOUT |  | Audio out
4 | VOUT |  | Composite Video out
5 | AIN |  | Audio in (into the SID chip)
6 | COLOR | - | Color ?
7 | n/c | - | Not connected
8 | +5VDC |  | +5 VDC

Note: Direction is Computer relative Monitor.

Contributor: | Joakim Ögren, Arwin Vosselman

Source: | CBM Memorial Page Pinouts
| SAMS Computerfacts CC8 Commodore 16

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10