# CBM 1902A

Available on the Commodore CBM 1902A monitor.

(at the Monitor)

6 PIN DIN FEMALE at the Monitor.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | n/c | - | Not connected
2 | AUDIO |  | Audio
3 | GND |  | Ground
4 | C |  | Chroma
5 | n/c | - | Not connected
6 | L |  | Luminance

Note: Direction is Monitor relative Computer.

Contributor: | Joakim Ögren

Source: | comp.sys.cbm General FAQ v3.1 Part 7

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10