# Mac to HP48

(at the Computer)
(to the HP48).

8 PIN MINI-DIN MALE to the Computer.
4 PIN ??? FEMALE to the HP48

| Mac | HP48 |
--- | --- | --- | ---
TxD- | 3 |  | RxD
RxD- | 5 |  | TxD
GND+RxD+ | 4+8 |  | GND
Shield | SHIELD | SHIELD | Shield

Contributor: | Joakim Ögren, Pierre Olivier

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13