# Atari Enhanced Joystick

Can be found at Atari Falcon, Jaguar & STe.

(at the computer)
(at the joystick cable)

15 PIN HIGHDENSITY D-SUB FEMALE at the computer.
15 PIN HIGHDENSITY D-SUB MALE at the joystick cable.

Pin | Name | Description
--- | --- | ---
1 | UP0 | Up 0
2 | DOWN0 | Down 0
3 | LEFT0 | Left 0
4 | RIGHT0 | Right 0
5 | PAD0Y | Paddle 0 Y
6 | FIRE0/LIGHT GUN | Fire 0/Lightgun
7 | VCC | +5 VDC
8 | n/c | Not connected
9 | GND | Ground
10 | FIRE2 | Fire 2
11 | UP2 | Up 2
12 | DOWN2 | Down 2
13 | LEFT2 | Left 2
14 | RIGHT2 | Right 2
15 | PAD0X | Paddle 0 X

Contributor: | Joakim Ögren

Source: | Atari Enhanced Joystick Ports FAQ

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10