# IndustrialPCI

PCI=Peripheral Component Interconnect.
IndustrialPCI is a version of PCI adapted for industrial and/or embedded applications.

The IPCI connector has three parts:

- Optional 60 pin PCI 64 bit extension (Top)
- Mandatory 120 pin PCI 32 bit (Middle)
- Optional 60 pin Custom I/O (Bottom)

(at the backplane)
(at the device (card))

UNKNOWN CONNECTOR at the backplane.
UNKNOWN CONNECTOR at the device (card).

## System Slot (Middle)

Pin | Name | Description | Note
--- | --- | --- | ---
A1 | +3,3V | +3.3 VDC |
A2 | AD2 | Address 2 |
A3 | AD6 | Address 6 |
A4 | GND | Ground |
A5 | AD10 | Address 10 |
A6 | AD13 | Address 13 |
A7 | GND | Ground |
A8 | SDONE | Snoop Done | 1
A9 | GND | Ground |
A10 | FRAME# | Indicate Address or Data phase | 1
A11 | AD18 | Address 18 |
A12 | GND | Ground |
A13 | +5V | +5 VDC |
A14 | AD24 | Address 24 |
A15 | AD27 | Address 27 |
A16 | GND | Ground |
A17 | REQ2 | Request 2 | 1
A18 | GND | Ground |
A19 | CLK1 | 33 or 66 MHz Clock |
A20 | CLK2 |  |
A21 | GND | Ground |
A22 | CLK3 |  |
A23 | CLK4 |  |
A24 | +3,3V | +3.3 VDC |
B1 | REQ64# | Request 64 ??? | 1
B2 | AD3 | Address 3 |
B3 | +5V | +5 VDC |
B4 | AD8 | Address 8 |
B5 | +3,3V | +3.3 VDC |
B6 | AD14 | Address 14 |
B7 | PAR | Parity |
B8 | +3,3V | +3.3 VDC |
B9 | STOP# | Stop | 1
B10 | C/BE2# | Command, Byte Enable 2 |
B11 | V(I/O) | +3.3 or +5 VDC |
B12 | AD21 | Address 21 |
B13 | +3,3V | +3.3 VDC |
B14 | V(I/O) | +3.3 or +5 VDC |
B15 | AD28 | Address 28 |
B16 | AD31 | Address 31 |
B17 | +3,3V | +3.3 VDC |
B18 | GNT3 | Grant 3 |
B19 | RST# | Reset |
B20 | NMI# | Non Maskable Interrupt |
B21 | X6 | Reserved (6) |
B22 | +5V | +5 VDC | :
B23 | RSTIN# |  | 2
B24 | USB+ | Universal Serial Bus (USB)(+) |
C1 | ACK64# | Acknowledge 64 ??? | 1
C2 | GND | Ground |
C3 | AD7 | Address 7 |
C4 | AD9 | Address 9 |
C5 | AD11 | Address 11 |
C6 | GND | Ground |
C7 | SERR# | System Error | 1
C8 | PERR# | Parity Error | 1
C9 | DEVSEL# | Device Select | 1
C10 | GND | Ground |
C11 | AD19 | Address 19 |
C12 | AD22 | Address 22 |
C13 | GND | Ground |
C14 | AD25 | Address 25 |
C15 | GND | Ground |
C16 | X1 | Reserved (1) |
C17 | GNT2 | Grant 2 |
C18 | REQ4 | Request 4 | 1
C19 | SLEEP#/SDAT | Sleep/Serial Data (I2C) | 3
C20 | X4 | Reserved (4) |
C21 | INTD# | Interrupt D | 1
C22 | INTB# | Interrupt B | 1
C23 | +5V | +5 VDC |
C24 | USB- | Universal Serial Bus (USB)(-) |
D1 | AD0 | Address 0 |
D2 | AD4 | Address 4 |
D3 | C/BE0# | Command, Byte Enable 0 |
D4 | +3,3V | +3.3 VDC |
D5 | AD12 | Address 12 |
D6 | AD15 | Address 15 |
D7 | V(I/O) | +3.3 or +5 VDC |
D8 | LOCK# | Resource Lock | 1
D9 | TRDY# | Test Logic Ready | 1
D10 | AD16 | Address 16 |
D11 | AD20 | Address 20 |
D12 | +5V | +5 VDC |
D13 | +5V | +5 VDC |
D14 | AD26 | Address 26 |
D15 | AD29 | Address 29 |
D16 | REQ1 | Request 1 | 1
D17 | REQ3 | Request 3 | 1
D18 | V(I/O) | +3.3 or +5 VDC |
D19 | X2 | Reserved (2) |
D20 | X5 | Reserved (5) |
D21 | +3,3V | +3.3 VDC |
D22 | INTA# | Interrupt A | 1
D23 | ICPEN#/SCLK | ICPEN/Serial Clock (I2C) | 3
D24 | OSC (PWDN) |  |
E1 | AD1 | Address 1 |
E2 | AD5 | Address 5 |
E3 | GND | Ground |
E4 | M66EN | Enable 66Mhz PCI-bus |
E5 | GND | Ground |
E6 | C/BE1# | Command, Byte Enable 1 |
E7 | SBO# | Snoop Backoff | 1
E8 | +5V | +5 VDC |
E9 | IRDY# | Initiator Ready | 1
E10 | AD17 | Address 17 |
E11 | GND | Ground |
E12 | AD23 | Address 23 |
E13 | C/BE3# | Command, Byte Enable 3 |
E14 | GND | Ground |
E15 | AD30 | Address 30 |
E16 | GNT1 | Grant 1 |
E17 | +5V | +5 VDC |
E18 | GNT4 | Grant 4 |
E19 | X3 | Reserved (3) |
E20 | GND | Ground |
E21 | INTC# | Interrupt C | 1
E22 | -12V | -12 VDC |
E23 | +12V | +12 VDC |
E24 | VBATT |  |

1 = Pullup resistor of 2,7 kOhm on the System Slot (CPU).
2 = Pullup resistor of 330 ohm on the System Slot (CPU).
3 = Pullup resistor of 4,7 KB ohm, if not supported by the System Slot (CPU).

## Module Bus Slot (Middle)

Pin | Name | Description | Note
--- | --- | --- | ---
A1 | +3,3V | +3.3 VDC |
A2 | AD2 | Address 2 |
A3 | AD6 | Address 6 |
A4 | GND | Ground |
A5 | AD10 | Address 10 |
A6 | AD13 | Address 13 |
A7 | GND | Ground |
A8 | SDONE | Snoop Done | 1
A9 | GND | Ground |
A10 | FRAME# | Indicate Address or Data phase | 1
A11 | AD18 | Address 18 |
A12 | GND | Ground |
A13 | +5V | +5 VDC |
A14 | AD24 | Address 24 |
A15 | AD27 | Address 27 |
A16 | GND | Ground |
A17 | REQ2 | Request 2 | 1
A18 | CLKM |  |
A19 | CLK1 | 33 or 66 MHz Clock |
A20 | CLK2 |  |
A21 | GND | Ground |
A22 | CLK3 |  |
A23 | CLK4 |  |
A24 | +3,3V | +3.3 VDC |
B1 | REQ64# | Request 64 ??? | 1
B2 | AD3 | Address 3 |
B3 | +5V | +5 VDC |
B4 | AD8 | Address 8 |
B5 | +3,3V | +3.3 VDC |
B6 | AD14 | Address 14 |
B7 | PAR | Parity |
B8 | +3,3V | +3.3 VDC |
B9 | STOP# | Stop | 1
B10 | C/BE2# | Command, Byte Enable 2 |
B11 | V(I/O) | +3.3 or +5 VDC |
B12 | AD21 | Address 21 |
B13 | +3,3V | +3.3 VDC |
B14 | V(I/O) | +3.3 or +5 VDC |
B15 | AD28 | Address 28 |
B16 | AD31 | Address 31 |
B17 | +3,3V | +3.3 VDC |
B18 | GNT3 | Grant 3 |
B19 | RST# | Reset |
B20 | NMI# | Non Maskable Interrupt |
B21 | X6 | Reserved (6) |
B22 | +5V | +5 VDC | :
B23 | RSTIN# |  |
B24 | USB+ | Universal Serial Bus (USB)(+) |
C1 | ACK64# | Acknowledge 64 ??? | 1
C2 | GND | Ground |
C3 | AD7 | Address 7 |
C4 | AD9 | Address 9 |
C5 | AD11 | Address 11 |
C6 | GND | Ground |
C7 | SERR# | System Error | 1
C8 | PERR# | Parity Error | 1
C9 | DEVSEL# | Device Select | 1
C10 | GND | Ground |
C11 | AD19 | Address 19 |
C12 | AD22 | Address 22 |
C13 | GND | Ground |
C14 | AD25 | Address 25 |
C15 | GND | Ground |
C16 | X1 | Reserved (1) |
C17 | GNT2 | Grant 2 |
C18 | REQ4 | Request 4 | 1
C19 | SLEEP#/SDAT | Sleep/Serial Data (I2C) |
C20 | X4 | Reserved (4) |
C21 | INTD# | Interrupt D | 1
C22 | INTB# | Interrupt B | 1
C23 | +5V | +5 VDC |
C24 | USB- | Universal Serial Bus (USB)(-) |
D1 | AD0 | Address 0 |
D2 | AD4 | Address 4 |
D3 | C/BE0# | Command, Byte Enable 0 |
D4 | +3,3V | +3.3 VDC |
D5 | AD12 | Address 12 |
D6 | AD15 | Address 15 |
D7 | V(I/O) | +3.3 or +5 VDC |
D8 | LOCK# | Resource Lock | 1
D9 | TRDY# | Test Logic Ready | 1
D10 | AD16 | Address 16 |
D11 | AD20 | Address 20 |
D12 | +5V | +5 VDC |
D13 | +5V | +5 VDC |
D14 | AD26 | Address 26 |
D15 | AD29 | Address 29 |
D16 | REQ1 | Request 1 | 1
D17 | REQ3 | Request 3 | 1
D18 | V(I/O) | +3.3 or +5 VDC |
D19 | X2 | Reserved (2) |
D20 | X5 | Reserved (5) |
D21 | +3,3V | +3.3 VDC |
D22 | INTA# | Interrupt A | 1
D23 | ICPEN#/SCLK | ICPEN/Serial Clock (I2C) | 3
D24 | OSC (PWDN) |  |
E1 | AD1 | Address 1 |
E2 | AD5 | Address 5 |
E3 | GND | Ground |
E4 | M66EN | Enable 66Mhz PCI-bus |
E5 | GND | Ground |
E6 | C/BE1# | Command, Byte Enable 1 |
E7 | SBO# | Snoop Backoff | 1
E8 | +5V | +5 VDC |
E9 | IRDY# | Initiator Ready | 1
E10 | AD17 | Address 17 |
E11 | GND | Ground |
E12 | AD23 | Address 23 |
E13 | C/BE3# | Command, Byte Enable 3 |
E14 | GND | Ground |
E15 | AD30 | Address 30 |
E16 | GNT1 | Grant 1 |
E17 | +5V | +5 VDC |
E18 | GNT4 | Grant 4 |
E19 | X3 | Reserved (3) |
E20 | GND | Ground |
E21 | INTC# | Interrupt C | 1
E22 | -12V | -12 VDC |
E23 | +12V | +12 VDC |
E24 | VBATT |  |

1 = Pullup resistor of 2,7 kOhm on the System Slot (CPU).

## Card Slot (Middle)

Pin | Name | Description | Note
--- | --- | --- | ---
A1 | +3,3V | +3.3 VDC |
A2 | AD2 | Address 2 |
A3 | AD6 | Address 6 |
A4 | GND | Ground |
A5 | AD10 | Address 10 |
A6 | AD13 | Address 13 |
A7 | GND | Ground |
A8 | SDONE | Snoop Done | 1
A9 | GND | Ground |
A10 | FRAME# | Indicate Address or Data phase | 1
A11 | AD18 | Address 18 |
A12 | GND | Ground |
A13 | +5V | +5 VDC |
A14 | AD24 | Address 24 |
A15 | AD27 | Address 27 |
A16 | GND | Ground |
A17 | IDSEL0 | IDSEL0 | 1
A18 | GND | Ground |
A19 | CLK1 | 33 or 66 MHz Clock |
A20 | GND | Ground |
A21 | GND | Ground |
A22 | GND | Ground |
A23 | GND | Ground |
A24 | +3,3V | +3.3 VDC |
B1 | REQ64# | Request 64 ??? | 1
B2 | AD3 | Address 3 |
B3 | +5V | +5 VDC |
B4 | AD8 | Address 8 |
B5 | +3,3V | +3.3 VDC |
B6 | AD14 | Address 14 |
B7 | PAR | Parity |
B8 | +3,3V | +3.3 VDC |
B9 | STOP# | Stop | 1
B10 | C/BE2# | Command, Byte Enable 2 |
B11 | V(I/O) | +3.3 or +5 VDC |
B12 | AD21 | Address 21 |
B13 | +3,3V | +3.3 VDC |
B14 | V(I/O) | +3.3 or +5 VDC |
B15 | AD28 | Address 28 |
B16 | AD31 | Address 31 |
B17 | +3,3V | +3.3 VDC |
B18 | GND | Ground |
B19 | RST# | Reset |
B20 | NMI# | Non Maskable Interrupt |
B21 | X6 | Reserved (6) |
B22 | +5V | +5 VDC | :
B23 | RSTIN# |  |
B24 | USB+ | Universal Serial Bus (USB)(+) |
C1 | ACK64# | Acknowledge 64 ??? | 1
C2 | GND | Ground |
C3 | AD7 | Address 7 |
C4 | AD9 | Address 9 |
C5 | AD11 | Address 11 |
C6 | GND | Ground |
C7 | SERR# | System Error | 1
C8 | PERR# | Parity Error | 1
C9 | DEVSEL# | Device Select | 1
C10 | GND | Ground |
C11 | AD19 | Address 19 |
C12 | AD22 | Address 22 |
C13 | GND | Ground |
C14 | AD25 | Address 25 |
C15 | GND | Ground |
C16 | X1 | Reserved (1) |
C17 | IDSEL1 | Initialization Device Select 1 |
C18 | GND | Ground |
C19 | SLEEP#/SDAT | Sleep/Serial Data (I2C) |
C20 | X4 | Reserved (4) |
C21 | INTD# | Interrupt D | 1
C22 | INTB# | Interrupt B | 1
C23 | +5V | +5 VDC |
C24 | USB- | Universal Serial Bus (USB)(-) |
D1 | AD0 | Address 0 |
D2 | AD4 | Address 4 |
D3 | C/BE0# | Command, Byte Enable 0 |
D4 | +3,3V | +3.3 VDC |
D5 | AD12 | Address 12 |
D6 | AD15 | Address 15 |
D7 | V(I/O) | +3.3 or +5 VDC |
D8 | LOCK# | Resource Lock | 1
D9 | TRDY# | Test Logic Ready | 1
D10 | AD16 | Address 16 |
D11 | AD20 | Address 20 |
D12 | +5V | +5 VDC |
D13 | +5V | +5 VDC |
D14 | AD26 | Address 26 |
D15 | AD29 | Address 29 |
D16 | REQ1 | Request 1 | 1
D17 | IDSEL2 | Initialization Device Select 2 |
D18 | V(I/O) | +3.3 or +5 VDC |
D19 | X2 | Reserved (2) |
D20 | X5 | Reserved (5) |
D21 | +3,3V | +3.3 VDC |
D22 | INTA# | Interrupt A | 1
D23 | ICPEN#/SCLK | ICPEN/Serial Clock (I2C) | 3
D24 | OSC (PWDN) |  |
E1 | AD1 | Address 1 |
E2 | AD5 | Address 5 |
E3 | GND | Ground |
E4 | M66EN | Enable 66Mhz PCI-bus |
E5 | GND | Ground |
E6 | C/BE1# | Command, Byte Enable 1 |
E7 | SBO# | Snoop Backoff | 1
E8 | +5V | +5 VDC |
E9 | IRDY# | Initiator Ready | 1
E10 | AD17 | Address 17 |
E11 | GND | Ground |
E12 | AD23 | Address 23 |
E13 | C/BE3# | Command, Byte Enable 3 |
E14 | GND | Ground |
E15 | AD30 | Address 30 |
E16 | GNT1 | Grant 1 |
E17 | +5V | +5 VDC |
E18 | GNT4 | Grant 4 |
E19 | X3 | Reserved (3) |
E20 | GND | Ground |
E21 | INTC# | Interrupt C | 1
E22 | -12V | -12 VDC |
E23 | +12V | +12 VDC |
E24 | VBATT |  |

1 = Pullup resistor of 2,7 kOhm on the System Slot (CPU).

## 64-bit PCI (Top)

Pin | Name | Description | Note
--- | --- | --- | ---
A1 | GND | Ground |
A2 | X10 | Reserved (10) |
A3 | AD35 | Address 35 | 2
A4 | AD38 | Address 38 | 2
A5 | AD42 | Address 42 | 2
A6 | V(I/O) | +3.3 or +5 VDC |
A7 | V(I/O) | +3.3 or +5 VDC |
A8 | AD52 | Address 52 | 2
A9 | AD56 | Address 56 | 2
A10 | AD60 | Address 60 | 2
A11 | AD63 | Address 63 | 2
A12 | GND | Ground |
B1 | X7 | Reserved (7) |
B2 | GND | Ground |
B3 | AD36 | Address 36 | 2
B4 | AD39 | Address 39 | 2
B5 | AD43 | Address 43 | 2
B6 | AD46 | Address 46 | 2
B7 | AD49 | Address 49 | 2
B8 | AD53 | Address 53 | 2
B9 | AD57 | Address 57 | 2
B10 | AD61 | Address 61 | 2
B11 | GND | Ground |
B12 | C/BE6# | Command, Byte Enable 6 | 2
C1 | X8 | Reserved (8) |
C2 | AD32 | Address 32 | 2
C3 | GND | Ground |
C4 | AD40 | Address 40 | 2
C5 | AD44 | Address 44 | 2
C6 | GND | Ground |
C7 | GND | Ground |
C8 | AD54 | Address 54 | 2
C9 | AD58 | Address 58 | 2
C10 | GND | Ground |
C11 | PAR64 | Parity 64 ??? | 2
C12 | C/BE7# | Command, Byte Enable 7 | 2
D1 | X9 | Reserved (9) |
D2 | AD33 | Address 33 | 2
D3 | AD37 | Address 37 | 2
D4 | GND | Ground |
D5 | AD45 | Address 45 | 2
D6 | AD47 | Address 47 | 2
D7 | AD50 | Address 50 | 2
D8 | AD55 | Address 55 | 2
D9 | GND | Ground |
D10 | AD62 | Address 62 | 2
D11 | C/BE4# | Command, Byte Enable 4 | 2
D12 | X11 | Reserved (11) |
E1 | GND | Ground |
E2 | AD34 | Address 34 | 2
E3 | V(I/O) | +3.3 or +5 VDC |
E4 | AD41 | Address 41 | 2
E5 | GND | Ground |
E6 | AD48 | Address 48 | 2
E7 | AD51 | Address 51 | 2
E8 | GND | Ground |
E9 | AD59 | Address 59 | 2
E10 | V(I/O) | +3.3 or +5 VDC |
E11 | C/BE5# | Command, Byte Enable 5 | 2
E12 | X12 | Reserved (12) |

2 = Pullup resistor of 2,7 kOhm (5V bus system) or 8,2 kOhm (3,3V bus system) on the backplane.

## ISA96/AT96 (Bottom)

Pin | Name | Description | Note
--- | --- | --- | ---
A1 | RSTDRV |  |
A2 | IRQ9 | Interrupt 9 |
A3 | SD11 | Data 11 |
A4 | SD9 | Data 9 |
A5 | IOCHRDY |  | 1
A6 | IOW# | I/O Write |
A7 | SA15 | Address 15 |
A8 | CLK | Clock |
A9 | SA10 | Address 10 |
A10 | SA7 | Address 7 |
A11 | T/C |  |
A12 | SA2 | Address 2 |
B1 | SD15 | Data 15 |
B2 | SD13 | Data 13 |
B3 | SD3 | Data 3 |
B4 | SD1 | Data 1 |
B5 | SMEMW# | System Memory Write |
B6 | SA18 | Address 18 |
B7 | SA14 | Address 14 |
B8 | DACK6# | DMA Acknowledge 6 |
B9 | SA9 | Address 9 |
B10 | IRQ3 | Interrupt 3 |
B11 | IOCS16# | I/O 16-bit chip select | 1
B12 | SA1 | Address 1 |
C1 | SD7 | Data 7 |
C2 | SD5 | Data 5 |
C3 | SD10 | Data 10 |
C4 | SD8 | Data 8 |
C5 | AEN | Address Enable |
C6 | IOR# | I/O Read |
C7 | SA13 | Address 13 |
C8 | SA11 | Address 11 |
C9 | IRQ5 | Interrupt 5 |
C10 | SA6 | Address 6 |
C11 | SA4 | Address 4 |
C12 | IRQ11 | Interrupt 11 |
D1 | SD14 | Data 14 |
D2 | SD12 | Data 12 |
D3 | SD2 | Data 2 |
D4 | SD0 | Data 0 |
D5 | SMEMR# | System Memory Read |
D6 | SA17 | Address 17 |
D7 | REF# |  |
D8 | IRQ7 | Interrupt 7 |
D9 | SA8 | Address 8 |
D10 | MCS16# |  | 1
D11 | BALE |  |
D12 | SA0 | Address 0 |
E1 | SD6 | Data 6 |
E2 | SD4 | Data 4 |
E3 | 0WS |  | 1
E4 | SBHE# |  |
E5 | SA19 | Address 19 |
E6 | SA16 | Address 16 |
E7 | SA12 | Address 12 |
E8 | DRQ6 | DMA Request 6 |
E9 | IRQ4 | Interrupt 4 |
E10 | SA5 | Address 5 |
E11 | SA3 | Address 3 |
E12 | IRQ10 | Interrupt 10 |

1 = Pullup resistor must be integrated into the System Slot (CPU).

## VMEbus (Bottom)

Pin | Name | Description
--- | --- | ---
A1 | D0 | Data 0
A2 | D2 | Data 2
A3 | D12 | Data 12
A4 | D7 | Data 7
A5 | DS1# |
A6 | BR3# |
A7 | AM1 |
A8 | AM3 |
A9 | IACKOUT# |
A10 | A14 | Address 14
A11 | A12 | Address 12
A12 | A10 | Address 10
B1 | BBSY# |
B2 | D10 | Data 10
B3 | D5 | Data 5
B4 | D15 | Data 15
B5 | SYSRES# |
B6 | A23 | Address 23
B7 | A21 | Address 21
B8 | A19 | Address 19
B9 | A16 | Address 16
B10 | A6 | Address 6
B11 | A4 | Address 4
B12 | A2 | Address 2
C1 | D8 | Data 8
C2 | D3 | Data 3
C3 | D13 | Data 13
C4 | SYSCLK |
C5 | DS0# |
C6 | DTACK# |
C7 | AS# |
C8 | IACK# |
C9 | AM4 |
C10 | A13 | Address 13
C11 | A11 | Address 11
C12 | A9 | Address 9
D1 | D1 | Data 1
D2 | D11 | Data 11
D3 | D6 | Data 6
D4 | BG3OUT# |
D5 | WR# | Write
D6 | AM0 |
D7 | AM2 |
D8 | A18 | Address 18
D9 | A15 | Address 15
D10 | A5 | Address 5
D11 | A3 | Address 3
D12 | A1 | Address 1
E1 | D9 | Data 9
E2 | D4 | Data 4
E3 | D14 | Data 14
E4 | BERR# | Bus Error
E5 | AM5 |
E6 | A22 | Address 22
E7 | A20 | Address 20
E8 | A17 | Address 17
E9 | A7 | Address 7
E10 | IRQ5# | Interrupt 5
E11 | IRQ3# | Interrupt 3
E12 | A8 | Address 8

## ECB (Bottom)

Pin | Name | Description
--- | --- | ---
A1 | D5 | Data 5
A2 | D2 | Data 2
A3 | A4 | Data 4
A4 | A7 | Address 7
A5 | BAI |
A6 | 2F |
A7 | A10 | Address 10
A8 | INT# |
A9 | VCMOS |
A10 | PWRCLR# |
A11 | A13 | Address 13
A12 | RESET# | Reset
B1 | D0 | Data 0
B2 | D4 | Data 4
B3 | A1 | Address 1
B4 | WAIT# |
B5 | A17 | Address 17
B6 | IEO |
B7 | n/c | Not connected
B8 | DMARDY |
B9 | RD# | Read
B10 | IORQ# |
B11 | ? |
B12 | n/c | Not connected
C1 | D6 | Data 6
C2 | A0 | Address 0
C3 | A5 | Address 5
C4 | A16 | Address 16
C5 | A18 | Address 18
C6 | BAO |
C7 | M1# |
C8 | WR# |
C9 | n |
C10 | A12 | Address 12
C11 | A9 | Address 9
C12 | n/c | Not connected
D1 | D7 | Data 7
D2 | A2 | Address 2
D3 | A8 | Address 8
D4 | BUSRQ# |
D5 | A19 | Address 19
D6 | A11 | Address 11
D7 | NMI# | Non Maskable Interrupt
D8 | PF |
D9 | HALT# |
D10 | RFSH# |
D11 | MRQ# |
D12 | n/c | Not connected
E1 | D3 | Data 3
E2 | A3 | Address 3
E3 | A6 | Address 6
E4 | IEI |
E5 | D1 | Data 1
E6 | A14 | Address 14
E7 | n/c | Not connected
E8 | n/c | Not connected
E9 | DESLCT# |
E10 | A15 | Address 15
E11 | BUSAK# |
E12 | n/c | Not connected

## SMP16 (Bottom)

Pin | Name | Description
--- | --- | ---
A1 | NMI# | Non Maskable Interrupt
A2 | IRQ0# | Interrupt 0
A3 | D11 | Data 11
A4 | D9 | Data 9
A5 | RDYIN |
A6 | IOW# |
A7 | A15 | Address 15
A8 | CLK |
A9 | A10 | Address 10
A10 | A7 | Address 7
A11 | TC/EOP# |
A12 | A2 | Address 2
B1 | D15 | Data 15
B2 | D13 | Data 13
B3 | D3 | Data 3
B4 | D1 | Data 1
B5 | MEMW# |
B6 | A18 | Address 18
B7 | A14 | Address 14
B8 | DACKx# |
B9 | A9 | Address 9
B10 | IRQ3# | Interrupt 3
B11 | IOCS16# |
B12 | A1 | Address 1
C1 | D7 | Data 7
C2 | D5 | Data 5
C3 | D10 | Data 10
C4 | D8 | Data 8
C5 | BUSEN |
C6 | IOR# |
C7 | A13 | Address 13
C8 | A11 | Address 11
C9 | IRQ1# | Interrupt 1
C10 | A6 | Address 6
C11 | A4 | Address 4
C12 | IRQ4# | Interrupt 4
D1 | D14 | Data 14
D2 | D12 | Data 12
D3 | D2 | Data 2
D4 | D0 | Data 0
D5 | MEMR# |
D6 | A17 | Address 17
D7 | INTA# |
D8 | INT# |
D9 | A8 | Address 8
D10 | MECS16# |
D11 | ALE |
D12 | A0 | Address 0
E1 | D6 | Data 6
E2 | D4 | Data 4
E3 | MMIO# |
E4 | BHEN |
E5 | A19 | Address 19
E6 | A16 | Address 16
E7 | A12 | Address 12
E8 | DRQx# |
E9 | IRQ2# | Interrupt 2
E10 | A5 | Address 5
E11 | A3 | Address 3
E12 | IRQ5# | Interrupt 5

## Floppy/EIDE (Bottom)

Pin | Name | Description
--- | --- | ---
A1 | FDSEL1 | Floppy Select 1
A2 | FDSEL0 | Floppy Select 0
A3 | FDME1 | Floppy ?
A4 | DIR | Floppy Direction
A5 | STEP | Floppy Step
A6 | WRDATA | Floppy Write Data
A7 | WE | Floppy Write?
A8 | TRK0 | Floppy Track 0
A9 | WP | Floppy Write?
A10 | RDDATA | Floppy ?
A11 | HDSEL | Floppy HD Select
A12 | DSKCHG | Floppy DiskChange
B1 | DRVDEN1 | ?
B2 | DRVDEN0 | ?
B3 | IDECS3P# | IDE ?
B4 | IDEA2 | IDE ?
B5 | IDEIRQS | IDE ?
B6 | IDEPUS | IDE ?
B7 | IDEDRQP | IDE ?
B8 | IDED14 | IDE Data 14
B9 | IDED8 | IDE Data 8
B10 | IDED6 | IDE Data 6
B11 | IDED11 | IDE Data 11
B12 | IDED3 | IDE Data 3
C1 | FDME0 | Floppy Me?
C2 | INDX | Floppy Index
C3 | IDECS3S# | IDE ?
C4 | IDEA0 | IDE ?
C5 | IDEDAKS# | IDE ?
C6 | IDEIOR# | IDE ?
C7 | IDEDRQS | IDE ?
C8 | IDED1 | IDE Data 1
C9 | #IDERST | IDE ?
C10 | IDED10 | IDE Data 10
C11 | IDED4 | IDE Data 4
C12 | IDED2 | IDE Data 2
D1 | IDELEDS# | IDE LED ?
D2 | IDELEDP# | IDE LED ?
D3 | IDECS1S# | IDE ?
D4 | IDEIRQP | IDE ?
D5 | IDEPUP | IDE Pull Up ?
D6 | IDEIOW# | IDE ?
D7 | IDED15 | IDE Data 15
D8 | IDED13 | IDE Data 13
D9 | IDED7 | IDE Data 7
D10 | GND | Ground
D11 | GND | Ground
D12 | GND | Ground
E1 | GND | Ground
E2 | GND | Ground
E3 | IDECS1P# | IDE ?
E4 | IDEA1 | IDE ?
E5 | IDEDAKP# | IDE ?
E6 | IDEIORDY | IDE ?
E7 | IDED0 | IDE Data 0
E8 | IDED12 | IDE Data 12
E9 | IDED9 | IDE Data 9
E10 | IDED5 | IDE Data 5
E11 | GND | Ground
E12 | GND | Ground

## SCSI (Bottom)

Pin | Name | Description
--- | --- | ---
A1 | TERM |
A2 | GND | Ground
A3 | I/O# |
A4 | REQ# |
A5 | ATN# |
A6 | D8 | Data 8
A7 | D9 | Data 9
A8 | D10 | Data 10
A9 | D2 | Data 2
A10 | D4 | Data 4
A11 | DP0 |
A12 | GND | Ground
B1 | TERM |
B2 | GND | Ground
B3 | GND | Ground
B4 | GND | Ground
B5 | GND | Ground
B6 | GND | Ground
B7 | GND | Ground
B8 | GND | Ground
B9 | GND | Ground
B10 | GND | Ground
B11 | GND | Ground
B12 | GND | Ground
C1 | TERM |
C2 | GND | Ground
C3 | C/D# |
C4 | MSG# |
C5 | ACK# |
C6 | D12 | Data 12
C7 | DP1 | Data P1
C8 | D13 | Data 13
C9 | D1 | Data 1
C10 | D5 | Data 5
C11 | D7 | Data 7
C12 | GND | Ground
D1 | TERM |
D2 | GND | Ground
D3 | GND | Ground
D4 | GND | Ground
D5 | GND | Ground
D6 | GND | Ground
D7 | GND | Ground
D8 | GND | Ground
D9 | GND | Ground
D10 | GND | Ground
D11 | GND | Ground
D12 | GND | Ground
E1 | TERM |
E2 | GND | Ground
E3 | SEL# |
E4 | RST# |
E5 | BSY# |
E6 | D14 | Data 14
E7 | D15 | Data 15
E8 | D11 | Data 11
E9 | D0 | Data 0
E10 | D3 | Data 3
E11 | D6 | Data 6
E12 | GND | Ground

Contributor: | Joakim Ögren, Rob Gill

Source: | IndustrialPCI page at Standard Industrial PC Systems's (SIPS) homepage

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10