# Two-Wire Modem (9-25)

This cable should be used for DTE to DCE (for instance computer to modem) connections without hardware handshaking.

(To Computer).
(To Modem).

9 PIN D-SUB FEMALE to the Computer
25 PIN D-SUB MALE to the Modem

| Female | Male | Dir
--- | --- | --- | ---
Shield Ground |  | 1 |
Transmit Data | 3 | 2 |
Receive Data | 2 | 3 |
System Ground | 5 | 7 |
Jumper these: |  |  |
Request to Send | 7 |  |
Clear to Send | 8 |  |
Data Set Ready | 6 |  |
Carrier Detect | 1 |  |
Data Terminal Ready | 4 |  |
Request to Send |  | 4 |
Clear to Send |  | 5 |
Data Set Ready |  | 6 |
Carrier Detect |  | 8 |
Data Terminal Ready |  | 20 |

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10