# IDE

The IDE interface requires only one cable. All pins straight from 1 to 1, 2 to 2 and so on. The drives can be connected in any order. Only remember that one should be jumpered as Master and the other as Slave. If only one drive is used, jumper it as Single (if such a mode exists, or most common Master else).

    Controller         Drive 1 or 2   Drive 1 or 2
    +--+                   +--+            +--+
    |::|===================|::|============|::|  <-Pin 1
    |::|===================|::|============|::|
    |::|===================|::|============|::|
    |::|===================|::|============|::|
    |::|===================|::|============|::|
    |::|===================|::|============|::|
    |::|===================|::|============|::|
    +--+                   +--+            +--+

(to the Controller)
(to the Drive 1)
(to the Drive 2)

40 PIN IDC FEMALE to the Controller.
40 PIN IDC FEMALE to the Drive 1.
40 PIN IDC FEMALE to the Drive 2.

| Controller | Drive 1 | Drive 2
--- | --- | --- | ---
Wire 1-40 | 1-40 | 1-40 | 1-40

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10