# SNES Video

Available on the Nintendo SNES.

(at the SNES)
(at the video cable)

SNES A/V MALE CONNECTOR at the SNES.
SNES A/V FEMALE CONNECTOR at the video cable.

Pin | Name | Description
--- | --- | ---
1 | R | Red (Requires 200 uF in series)
2 | G | Green (Requires 200 uF in series)
3 | CSYNC | Composite Sync
4 | B | Blue (Requires 200 uF in series)
5 | GND | Ground
6 | GND | Ground
7 | Y | S-Video Y
8 | C | S-Video C
9 | CVBS | Composite Video
10 | +5V | +5 VDC
11 | L+R | Left+Right Audio (Mono)
12 | L-R | Left-Right Audio (Used to calculate Stereo)

Note: Pin 3 is SCART Switch voltage (+11 VDC) on PAL machines

Contributor: | Joakim Ögren, Mark K

Source: | Video Games FAQ (Part 3)
| Pinout from Radio Electronics April 1992
| SNES A/V Pinout at GamesX

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10