# Vic 20 Video

(at the computer)
(at the cable)

5 PIN DIN 180° (DIN41524) FEMALE at the Computer.
5 PIN DIN 180° (DIN41524) MALE at the Cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | +6V |  | +6 VDC (10 mA max)
2 | GND |  | Ground
3 | AUDIO |  | Audio
4 | VLOW |  | Video Low (Unconnected ?)
5 | VHIGH |  | Video High

Note: Direction is Computer relative Monitor.

Contributor: | Joakim Ögren

Source: | CBM Memorial Page Pinouts

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10