# Amiga to SCART

(to the Amiga)
(to the TV)

23 PIN D-SUB FEMALE to the Amiga
21 PIN SCART MALE to the TV

| Amiga | TV |
--- | --- | --- | ---
Analog Red | 3 | 15 | RGB Red In
Analog Green | 4 | 11 | RGB Green In
Analog Blue | 5 | 7 | RGB Blue In
Composite Sync | 10 | 20 | Video In
Video GND | 17 | 17 | Video GND
GND | 19 | 18 | Blanking GND
+12V | 22 | 16 | Blanking (Connect via a 150 Ohm resistor)
+12V | 22 | 8 | Audio/RGB switch (Connect via a 1 kOhm resistor)
Phono Right |  | 2 | Audio IN Right
Phono Right GND |  | 4 | GND
Phono Left |  | 6 | Audio IN Left
Phono Left GND |  | 4 | GND

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10