# Triplite OmniPro 675 UPS

Unknown connector

Pin | Description
--- | ---
1 | Common/Negative
2 | External inverter shutdown, positive side
3 | line fail, normaly open contact
4 | return/external inverter shutdown negative side
5 | line fail, normaly closed contact
6 | low battery, positive side (2 minute warning)

Contributor: | Joakim Ögren

Source: | Triplite OmniPro 675 UPS pinout at The Pin-Out directory

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10