# C64 Power Supply

Available at the Commodore 64.

(at the computer)

7 PIN DIN 'C' FEMALE at the computer.

Pin | Name | I C64 | I C64C
--- | --- | --- | ---
1 | Shield Ground |  |
2 | Shield Ground |  |
3 | Shield Ground |  |
4 | Not connected (or +5VDC In) |  |
5 | +5VDC In | 1.5A | 1.7A
6 | 9VAC in | 1.0A | 1.0A
7 | 9Vac in | 1.0A | 1.0A

Note: Max current from power supply is indicated above.

Contributor: | Rob Gill, Myles Williams

Source: | Commodore 64 Programmers Reference Guide
| NT Rautanen Tietokonesivut: Commodore

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13