# Monochrome TTL Video

(18.43 KHz - 720x350)

(At the videocard)
(At the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | - | -
3 | - | -
4 | - | -
5 | - | -
6 | I | Intensity
7 | VID | Video
8 | HSYNC | Horizontal Sync TTL Positive
9 | VSYNC | Vertical Sync TTL Negative

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13