# Atari 2600 Joystick

(at the Atari)
(at the joystick cable)

9 PIN D-SUB MALE at the Atari.
9 PIN D-SUB FEMALE at the joystick cable.

Pin | Color | Dir | Description
--- | --- | --- | ---
1 | WHT |  | Up
2 | BLU |  | Down
3 | GRN |  | Left
4 | BRN |  | Right
5 | n/c | - | Not connected
6 | ORG |  | Button
7 | n/c | - | Not connected
8 | BLK |  | Ground(-)
9 | n/c | - | Not connected

Note: Direction is Computer relative Joystick.
Note: Connect Direction/Button to Ground for action.

Contributor: | Joakim Ögren

Source: | Classic Atari 2600/5200/7800 Game Systems FAQ - Pinout by Greg Alt

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13