# Atari Mouse/Joy

(at the computer)
(at the mouse/joy cable)

9 PIN D-SUB MALE at the computer.
9 PIN D-SUB FEMALE at the mouse/joy cable.

Pin | Mouse | Joystick | Dir | Comment
--- | --- | --- | --- | ---
1 | XB | UP |  |
2 | XA | DOWN |  |
3 | YA | LEFT |  |
4 | YB | RIGHT |  |
5 | n/c | n/c | - |
6 | LEFTBUTTON | FIRE |  |
7 | +5V | +5V |  |
8 | GND | GND |  |
9 | RIGHTBUTTON | res |  |

Note: Direction is Computer relative Device.

Contributor: | Joakim Ögren, Steve & Sally Blair

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13