# NeoGeo Joystick

Available on the NeoGeo videogame.

(at the console)
(at the joystick cable)

15 PIN D-SUB FEMALE at the console.
15 PIN D-SUB MALE at the joystick cable.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND |  | Ground
2 | n/c | - | Not connected
3 | SELECT |  | Select Button
4 | BUTTOND |  | "D" Button
5 | BUTTONB |  | "B" Button
6 | RIGHT |  | Right
7 | DOWN |  | Down
8 | n/c | - | Not connected
9 | BUTTOND |  | "D" Button, again?
10 | n/c | - | Not connected
11 | START |  | Start Button
12 | BUTTONC |  | "C" Button
13 | BUTTONA |  | "A" Button
14 | LEFT |  | Left
15 | UP |  | Up

Note: Direction is Computer relative Joystick.
Note: Signals are active high (connect to +5V).

Contributor: | Joakim Ögren, Enzo

Source: | NeoGeo Controller pinout at GamesX

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10