# VHS Video Camera

10 PIN UNKNOWN CONNECTOR

          key
           ?
       1      8
           9            camera plug connector
    2            7      pins facing you
          10
    3            6

       4      5

There seems to be no clear standard for VHS Video Cameras. Column "Name" is the most common function. Three alternative functions that could apply for some cameras is presented in columns named "Alt Name X".

Pin | Name | Alt Name 1 | Alt Name 2 | Alt Name 3
--- | --- | --- | --- | ---
1 | video out | video in/out |  |
2 | video gnd |  |  |
3 |  | serial data |  |
4 |  | tally and clock | reset in |
5 |  | audio out right | standby out | audio in
6 | pause |  |  |
7 | audio out | audio out left |  |
8 | audio gnd |  |  |
9 | power gnd |  |  |
10 | +12V power |  |  |

Contributor: | Joakim Ögren, Mike Turner, Mike N3EZD

Source: | VHS Video Camera 10 pin pinout at Baltimore Radio Amateur Television Society
| Pinouts FAQ at Sci.Electronics.Repair FAQ

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10