# PC to HP48

(to the Computer).
(to the HP48).

9 PIN D-SUB FEMALE to the Computer.
4 PIN HP48 FEMALE to the HP48

| PC | HP48 |
--- | --- | --- | ---
Shield | SHIELD | 1 | Shield
RxD | 2 | 2 | RxD
TxD | 3 | 3 | TxD
GND | 5 | 4 | GND

Contributor: | Joakim Ögren, Frank Vorstenbosch, Andrew Chen

Source: | comp.sys.hp48 FAQ

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-14