# C64/128 Cassette

(at the computer)

6 PIN MALE EDGE at the computer.

Pin | Name | Dir | Description
--- | --- | --- | ---
A-1 | GND |  | Ground
B-2 | +5V |  | +5 Volts DC
C-3 | MOTOR |  | Cassette Motor
D-4 | READ |  | Cassette Read
E-5 | WRITE |  | Cassette Write
F-6 | SENSE |  | Cassette Sense

Note: Direction is Computer relative Cassette.

Contributor: | Joakim Ögren, Arwin Vosselman

Source: | Commodore 64 Programmer's Reference Guide

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13