# C128 Power Supply

Available at the Commodore 128.

(at the computer)

5 PIN SQUARE?? FEMALE at the computer.

Pin | Name | Description | I
--- | --- | --- | ---
1 | +5VDC | +5V DC | 2.5A
2 | n/c |  |
3 | 9VAC | 9V AC | 1.0A
4 | GND | Ground |
5 | 9VAC | 9V AC | 1.0A

Note: Max current from power supply is indicated above.

Contributor: | Joakim Ögren

Source: | NT Rautanen Tietokonesivut: Commodore

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13