# ParNet Parallel

(To Computer 1).
(To Computer 2).

25 PIN D-SUB MALE to Computer 1.
25 PIN D-SUB MALE to Computer 2.

Name | Pin | Pin | Name
--- | --- | --- | ---
Data Bit 0 | 2 | 2 | Data Bit 0
Data Bit 1 | 3 | 3 | Data Bit 1
Data Bit 2 | 4 | 4 | Data Bit 2
Data Bit 3 | 5 | 5 | Data Bit 3
Data Bit 4 | 6 | 6 | Data Bit 4
Data Bit 5 | 7 | 7 | Data Bit 5
Data Bit 6 | 8 | 8 | Data Bit 6
Data Bit 7 | 9 | 9 | Data Bit 7
Acknowledge + Select | 10+13 | 10+13 | Acknowledge + Select
Busy | 11 | 11 | Busy
Paper Out | 12 | 12 | Paper Out
Signal Ground | 17-25 | 17-25 | Signal Ground

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10