# 3.5" Power

Used for floppies.
Name according to the ATX standard: Floppy Drive Connector.

(at the powersupply cable)
(at the peripheral)

UNKNOWN CONNECTOR at the powersupply cable.
UNKNOWN CONNECTOR at the peripheral.

Pin | Name |  | Color | Description
--- | --- | --- | --- | ---
1 | +5V |  | Red | +5 VDC
2 | GND |  | Black | +5 V Ground
3 | GND |  | Black | +12 V Ground (Same as +5 V Ground)
4 | +12V |  | Yellow | +12 VDC

Recommended wiresize according to the ATX standard: 20 AWG
At cables: AMP 171822-4

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10