# Amstrad Digital Joystick

Available at the Amstrad CPC6128 and CPC6128 Plus.

(at the Computer)
(at the Joystick cable)

9 PIN D-SUB MALE at the Computer.
9 PIN D-SUB FEMALE at the Joystick cable.

## Digital Joystick 1

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | UP |  | Up
2 | DOWN |  | Down
3 | LEFT |  | Left
4 | RIGHT |  | Right
5 | n/c | - | Not connected
6 | FIRE2 |  | Fire button 2
7 | FIRE1 |  | Fire button 1
8 | GND |  | Ground
9 | GND |  | Ground

## Digital Joystick 2

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | UP |  | Up
2 | DOWN |  | Down
3 | LEFT |  | Left
4 | RIGHT |  | Right
5 | n/c | - | Not connected
6 | FIRE2 |  | Fire button 2
7 | FIRE1 |  | Fire button 1
8 | GND |  | Ground
9 | n/c | - | Not connected

Note: Direction is Computer relative Joystick.

Contributor: | Joakim Ögren, Colin Gaunt, Agnello Guarracino

Source: | Amstrad 6128 Plus Home Computer Manual Amstrad CPC6128 User Instructions Manual

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13