# SGI StereoView (3 pin)

(at the computer)

3 PIN MINI-DIN FEMALE at the computer.

Pin | Description
--- | ---
1 | STEREO POWER (+12V, 0.5A)
2 | STEREO GROUND
3 | VERTICAL - ODD FIELD (1=Left, 0=Right)

Contributor: | Joakim Ögren

Source: | SGI Indy Workstation Owner's Guide

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10