# DEC DLV11-J Serial

Available on the DEC DLV11-J Serial card

(at the serial card)

10 PIN IDC MALE at the Serial card.

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | CLK | ? | Clock
2 | GND |  | Ground
3 | TXD+ |  | Transmit data +
4 | TXD- |  | Transmit data - (0V for RS-232, Reader enable for 20mA)
5 | GND |  | Ground
6 | n/c | - | Not connected (no pin)
7 | RXD- |  | Receive data -
8 | RXD+ |  | Receive data +
9 | GND |  | Ground
10 | +12V |  | +12 VDC

Note: Direction is Serial card relative other Devices.

Contributor: | Ben Harris

Source: | DEC DLV11-J Printset, M8043-0-1, sheet 7

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10