# CGA

CGA=Color Graphics Adapter.
Videotype: TTL, 16 colors.
Also known as IBM RGBI.

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | GND | Ground
3 | R | Red
4 | G | Green
5 | B | Blue
6 | I | Intensity
7 | RES | Reserved
8 | HSYNC | Horizontal Sync
9 | VSYNC | Vertical Sync

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13