# Atari ST Monitor Connector

(at the Computer)
(at the Devices)

13 PIN DIN FEMALE at the Computer.
13 PIN DIN MALE at the Devices.

Pin | Name | Description
--- | --- | ---
1 | AO | Audio Out
2 | CVIDEO | Composite Video
3 | CS | Clock Select
4 | MD | Monochrome Detect / Clock In
5 | AI | Audio In
6 | G | Green
7 | R | Red
8 | +12V | +12 VDC (520ST has GND)
9 | HSYNC | Horizontal Sync
10 | B | Blue
11 | MVIDEO | Monochrome Video
12 | VSYNC | Vertical Sync
13 | GND | Ground

Contributor: | Joakim Ögren, Lawrence Wright, Steve & Sally Blair

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10