# Serial (15)

Seems to be available at a 14.4kbps modem called Speedster.

         2   4   6      10  12  14
    - [][][][][][][][][][][][][][][] -
       1   3   5   7 8 9  11  13  15

(at the modem)

15 PIN FEMALE ??? at the modem.

Pin | Name | RS232 | Dir | Description
--- | --- | --- | --- | ---
1 | GROUND | GND |  | Ground
2 | SUSP# |  | ? |
3 | COMBDSR# | DSR |  | Data Set Ready
4 | COMBRTS# | RTS |  | Request to Send
5 | COMBCTS# | CTS |  | Clear to Send
6 | COMBRI# | RI |  | Ring Indicator
7 | n/c |  | ? |
8 | GROUND | GND |  | Ground
9 | +5VIN |  |  | +5V DC In
10 | COMBDTR# | DTR |  | Data Terminal Ready
11 | COMBDCD# | CD |  | Carrier Detect
12 | COMBTXD | TXD |  | Transmit Data
13 | COMBRXD | RXD |  | Receive Data
14 | SPKDATA |  | ? |
15 | GROUND | GND |  | Ground

Contributor: | Joakim Ögren, Joerg Brinkel

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10