# Misc Unsupported Cables

These cables may or may not be correctly constructed. Handle with care.

# Amiga to IBM RGBI Cable

(to the Monitor).
(to the Amiga).

9 PIN D-SUB ?? to the Monitor.
23 PIN D-SUB FEMALE to the Amiga.

| 9 Pin | 23 Pin | Comment
--- | --- | --- | ---
Ground | 1 | 16 |
Ground | 2 | 16 |
Digital Red | 3 | 9 | (Via 2 Hex Inverters, i.e 74LS04)
Digital Green | 4 | 8 | (Via 2 Hex Inverters, i.e 74LS04)
Digital Blue | 5 | 9 | (Via 2 Hex Inverters, i.e 74LS04)
Digital Intensity | 6 | 6 | (Via 2 Hex Inverters, i.e 74LS04)
Horizontal Sync | 8 | 11 | (Via 1 Hex Inverters, i.e 74LS04)
Verical Sync | 9 | 12 | (Via 1 Hex Inverters, i.e 74LS04)
+5V |  | 23 | (Power for the IC)

# C128 80 columns to 1702 monitor Cable

(to the C128).
(to the C1702).

9 PIN D-SUB MALE to the C128.
PHONO MALE to the Monitor.

| C128 | C1702 |
--- | --- | --- | ---
Ground | 1 | 1 | Ground
Monochrome out | 7 | 2 | Signal

Contributor: | Joakim Ögren

Source: | Gordon

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10