# Panasonic G500

UNKNOWN CONNECTOR

Pin | Name | Dir | Description
--- | --- | --- | ---
1 | GND | --- | Ground
2 | TX_Audio | --> | ?
3 | AGND | --- | Audio_Ground
4 | HF_ON (L=ON) | --> | L=H/F ON
5 | AOP_Sense | <-- | Data Adaptor Select
6 | Serial_Up | <-- | UART up (9600,33.8kbps)
7 | Serial_Down | --> | UART down
8 | External_Power | <-- | POWER FOR CHARGING
9 | Ground |  |
10 | RX_Audio | <-- |
11 | Radio_Mute | --> | L=MUTE
12 | HF_Sense | <-- | L=H/F MODE
13 | Reserved |  | L=FLASH WRITE ENABLE
14 | Ignition | <-- | H=ON
15 | Logic_Power | --> | H=HANDSET ON
16 | PAON | --> | Power Amplifier Control Signal

Contributor: | Joakim Ögren

Source: | Panasonic G500 pinout at Technick.net

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10