# MDA (Hercules)

(at the videocard)
(at the monitor cable)

9 PIN D-SUB FEMALE at the videocard.
9 PIN D-SUB MALE at the monitor cable.

Pin | Name | Description
--- | --- | ---
1 | GND | Ground
2 | GND | Ground
3 | n/c |
4 | n/c |
5 | n/c |
6 | I | Intensity
7 | M | Mono Video
8 | H | Horizontal Sync
9 | V | Vertical Sync

Contributor: | Joakim Ögren

Source: | ?

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-13