# ParaLoad

(To C64).
(To Amiga).

DZM 12 DREH at the C64 UserPort.
25 PIN D-SUB MALE at the Amiga

| C64 | Amiga |
--- | --- | --- | ---
Ground | A | 17-25 | Ground
FLAG2 | B | 1 | Strobe
PB0 | C | 2 | D0
PB1 | D | 3 | D1
PB2 | E | 4 | D2
PB3 | F | 5 | D3
PB4 | H | 6 | D4
PB5 | J | 7 | D5
PB6 | K | 8 | D6
PB7 | L | 9 | D7
PA2 | M | 11 | Busy

Contributor: | Joakim Ögren

Source: | ParaLoad documentation

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10