# S-Video to Composite

Use this cable to connect a S-Video output to a composite video input.

(to the Video Source)
(to the TV/Monitor)

4 PIN MINI-DIN FEMALE at the peripheral. PHONO MALE to the Monitor-cable.

Description | S-Video | Composite | Dir
--- | --- | --- | ---
Y Ground | 1 | ground |
C ground | 2 | ground |
Y (luminance+sync) | 3 | signal |
C (crominance) | 4 | signal (470pF capacitor) |

Note: Use signal 470pF ceramic capacitor (rated 10V).

Contributor: | Joakim Ögren

Source: | Tomi Engdahl's pages at ePanorama

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2004-01-12