# Apple IIc Joystick

9 PIN UNKNOWN CONNECTOR

Pin | Name | Description
--- | --- | ---
1 | GAMESW1 | Switch input 1 (sometimes called paddle button 1).
2 | +5V | +5 VDC (max 100mA)
3 | GND | System ground.
4 | n/a | Not used
5 | PDL0 | Paddle 0 hand controller input. Must be connected to a 150K ohm variable resistor connected to +5V.
6 | n/c | Not connected
7 | GAMESW0 | Switch input 0 (sometimes called paddle button 0).
8 | PDL1 | Paddle 1 hand controller input; must be connected to a 150K ohm variable resistor connected to +5V.
9 | n/a | Not used

Contributor: | Joakim Ögren

Source: | Apple Tech Info Library 1419: Apple IIc, External Pinouts at Apple TIL homepage

Copyright © The Hardware Book Team 1996-2004.
May be copied and redistributed, partially or in whole, as appropriate.
Document last modified: 2002-01-10