Video Output

This is XL/XE monitor output connector. Note: this info is incomplete, some models are lacking certain outputs. From FAQ:
400 and 600XL completely lack monitor port.
XL line lacks separate chroma signal. (Contradicts previous statement for 600XL)
XEGS has only RCA jack (with composite video).
XEP80 has RCA jack (with composite video).

1 | composite luminance
2 | gnd
3 | audio out
4 | composite video
5 | composite chrominance

This is XL/XE monitor output for SECAM based Ataris.

1 | +12V DC 5mA
2 | audio 1 out
3 | audio 2 out
4 | video out
5 | gnd
6 | +5V 100mA

Back (c) 1998-2004 Jindroush Last modified: Mon Oct 7 00:23:12 2002