
  Hard disk image file
for usage with Atari ST(E) computers
or Atari emulators.

  Main image is with ACSI autoboot
driver. So, will boot on any Atari ST(E)
machine equipped with some hard disk
attached onto ACSI port via adapter.
And with Satandisk, Ultrasatan too.

  If have IDE hard disk or CF card on IDE
port still may autoboot, only needs to over-
write disk begin with suplied 1GB_IDE.IMG.



  PP. March 2010
 