In this directory you'll find latest version of VBXE cores

VBXE 2.1 users have them already installed (except Atari 5200 related ones), and VBXE 2.0 and 1.x 
users will have to install then using FC.COM

For those of you who have SIDE or SIDE-2 cartridge i suggest to upgrade it first, so you would have CIO
over FAT32 and FC.COM will work directly of FAT32/16 directory

Here is naming convention we've used:

v_versionnumber_coretype_version_suffix

suffixes:
a - plain core, w/o memory expansion emulation
r - core with rambo memory expansion emulation
g - core for Atari 5200

ie:
 v1fx126a - vbxe 1.x core FX version 1.26 w/o memory expansion emulation
 v2g106g  - vbxe 2.x core GTIA version 1.06 for Atari 5200
 v2fx126r - vbxe 2.x core FX version 1.26 with rambo memory expansion emulation

etc...

FC.COM won't allow you to load VBXE 1.x core into 2.x hardware and vice versa, so do not worry too much


VBXE Team

